Icom 207H Dual Band Mobil.....
I have preformed this mod on my 2 207H mobil's with success, but doing this
mod is AT YOUR OWN RISK.....

remove the 4 screws ataching the bottom cover and remove the cover. (I had to
 use a small screwdriver to pry on the cover. It's made to fit tight)
with face toward you and belly up look to far right of board and close to you
locate a row of SMT diodes 3 on top then a shift to right and a few more.
The three are in a PERFECT row top to bottom! count from the top of the row
1 2 3. Remove the # 2 & 3 diodes. Now continue looking down from there and
you will see a resistor sticking up in the air (W14). Clip the lead off of
the resistor. Reassemble the radio  and preform a CPU reset by holding the
Set and S.MW buttons while turning the radio on...(page 69 of manual).

You now will have :

	118-135 RX  (stock)
	136-174 TX & RX
	320-399 RX  (hmmm whats there? I've heard a local radio station DJ
		     at a remote location talking to the station)
	400-479 TX & RX
	849-950 RX

The Transmitter will work and transmit at ALL of the listed TX freqs. and the
power seems to be fairly broad banded and can handle it...
I now use my mobils as Ham AND GMRS. One less piece to lug around!

