
        INTERFACING ICOM IC-32(A/AT/E) AND 9600 BAUD MODEM
        --------------------------------------------------

IC706 and IC707 are locate on the bottom of then MAIN UNIT (first card you 
see after removing of the back alluminium-cover of the IC32).

Componenst must be located reading the reference on its package.


                    C798 (.0022)      |       |
                  ____||______________|6     3|__     
        R765(82k) |   ||              |       |    IC706 (M5218FP)
      ____/\/\/\__|____/\/\/\_________|5     4|__   
                      R766 (82K)  |   |_______|
                 /|\            __|__ 
                  |             _____ C800 (120)
                  |               |   
                  |               |     
                  |              GND
              In 9k6 (out from modem) to the VCO varactor.

Discriminator output is taken directly from pin 11 of IC707 (TK10420M)
and put into 9K6 modem input.

PTT is connected directly to the ptt key (J710).


