
Modification for HAM band
Author: amtu_ok@yahoo.com

If your radio can't TX on HAM band, you may try these steps below:
1. Turn off radio and opened 9 screws on back side.
2. Turn radio up side down until you see fan and the bigger PCB number B4248K. On the right side of PCB find IC number TD62783AF. On the left side of the IC find 7 diodes number D201-D207.
3. Cut diode number D203-D206, and reinstall the cabinet carefully.


Modification for 120W on 10m band.
Author: Domenico Lindo

I have been modified my marine transceiver IC-M710 to get full power on 10m band that is normally reduced for this marine transceiver.
To do the modification it is necessary remove D59.