Knowledge Base Article 5ATG175622 

Issue
My 706 won't power up.

Resolution
You may have a burned ground circuit trace in the flex cable. Replace the flex cable (EP2) at the mainboard.

Category
Amateur : HF : 706