Knowledge Base Article 5ATF636377 

Issue
My 706 has low TX output on HF and 6 meters.

Resolution
There is probably a shorted D18 diode and Q1 transistor in filter unit. Replace D18 diode (DAP222) and Q1 transistor (2SC4081). 
