Knowledge Base Article 5ATF692714 

Issue
My 706 has low microphone gain.

Resolution
Change the value of R236 resistor from 27k to 68k-82k. The higher the resistor value, the greater increase in mic gain.

Category
Amateur : HF : 706