Knowledge Base Article 5ATG116282 

Issue
My 706 is off frequency in FM TX. Other modes OK.

Resolution
FM VCO lock voltage needs adjustment. Adjust FM VCO lock voltage for 1.5 volts as per service manual. 

Category
Amateur : HF : 706