Knowledge Base Article 5ATF57195A 

Issue
My 706 has no TX power output on one or two HF bands.

Resolution
There's a bad filter relay. Locate and replace faulty filter relay (will be type AHY-103) on the filter circuit board.

Category
Amateur : HF : 706