tx Mod For ICOM 735

The mod for gen/cov tx for the IC-735 involves removing D33 and D34 from
the main board. You'll have to lift the PA module up to do this, locate the
diodes and simply snip one end of each. Very simple, but it's amazing just
how many screws need removing in the process!

Good luck,
Simon Browne G0GWA.
================================================================
