
Date: 18 Sep 89 08:39:55 GMT
From: ka9q.bellcore.com!karn@bellcore.com  (Phil Karn)
Subject: Local packet QSOs / dual band rigs?

The receiver recovery time with that radio is overly long. 
The fix is simple: open up the rig and remove diode
D19 in the audio output stage. This diode biases the output stage off
during transmit, but it is unnecessary because there are other audio
gates ahead of this stage.

Phil
