HERE IS SOMTHING YOU CAN DO IF YOUR
DIGITAL DISPLAY ON THE KENWOOD TS-820
IS GIVING YOU A PROBLEM..............

 1 -- REMOVE THE COUNTER ASSEMBLY UNIT FROM THE 820.

 2 -- REMOVE BOTH CIRCUIT BOARDS FROM THE COUNTER ASSEMBLY
 (UPPER AND LOWER BOARDS).

 3 -- SCRAPE AWAY THE VARNISH FROM THE CORNERS OF THE BOARDS WHERE THE 
INTERCONNECTING SCREWES AND SPACERS HOLD THE BOARDS INTO THE CASE.

 4-- REASSEMBLE THE COUNTER....

 THAT SHOULD TAKE CARE OF THE PROBLEM..

 GOOD LUCK......

 BY--K0HRF............RELAYED  BY...N0KGX...GENE


 
 73S DE JERONIMO  EA7FHR @EA7FKB.EAAL.ESP.EU.
